# no area

#### Syntax

no area { areaId | areaIdInt }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Removes the specified OSPF area if there are no OSPF interfaces configured in the area. This command has only a no version.

#### Options

- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value in the range 0–4294967295

#### Mode

Router Configuration