# aaa tunnel switch-profile

#### Syntax

aaa tunnel switch-profile profileName

no aaa tunnel switch-profile

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Applies a default L2TP tunnel switch profile to a virtual router. The default tunnel switch profile defines the L2TP tunnel switching behavior for the interfaces to which this profile is assigned. The router uses the default tunnel switch profile if the tunnel attributes returned from an AAA domain map or tunnel group or from a RADIUS authentication server do not include a named tunnel switch profile. The no version removes the default tunnel switch profile assignment from the virtual router.

#### Options

- profileName—Name of the default tunnel switch profile; a string of up to 64 alphanumeric characters

#### Mode

Global Configuration