# aaa tunnel nas-port-method

#### Syntax

aaa tunnel nas-port-method cisco-avp

no aaa tunnel nas-port-method

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the tunnel's default NAS port type to provide limited support for a Cisco proprietary vendor-specific method when configuring the LAC to LNS NAS port identification transfer mechanism. The no version disables the command.

| Note: Use of this feature is not recommended and continued compatibility cannot be guaranteed.

#### Mode

Global Configuration