# aps working

#### Syntax

aps working [ 1 ]

no aps working

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an interface as a working interface. The no version removes the configuration.

#### Options

- 1—Channel number that identifies the working interface; because the working interface is always assigned channel number 1, this is the only valid option

#### Mode

Controller Configuration