# warning

#### Syntax

warning maximumUtilization minimumUtilization

no warning

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the minimum and maximum threshold values for DHCP local address pool utilization. If you issue the snmp-server command, SNMP traps are generated when utilization occurs above or below the specified threshold values. The no version restores the default threshold values for local address pool utilization.

#### Options

- maximumUtilization—Maximum utilization value for the DHCP local address pool
- minimumUtilization—Minimum utilization value for the DHCP local address pool

#### Mode

DHCP Local Pool Configuration