# bandwidth

#### Syntax

bandwidth bandwidth

no bandwidth

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the total bandwidth available on the interface. For total reservable bandwidth, see the mpls bandwidth command. The no version removes the admission control configuration from the interface.

#### Options

- bandwidth—Available bandwidth in kilobits per second, a value from 1–10,000,000

#### Mode

Interface Configuration, Subinterface Configuration

#### Related Documentation

- ospf bandwidth