# Example: Simple Shared Shaping for Ethernet

In a typical triple-play network configuration over Ethernet, individual subscribers are represented on the B-RAS by VLANs and DSLAMs by SVLANs. In this example, the provider shapes the subscriber aggregate of voice, video, and data to a single rate.

In this example, S-VLAN 0 has traffic in three traffic-class groups: the default group, the TC1 traffic class in the G1 group, and the TC2 traffic class in the G2 traffic-class group.

Figure 21: Hierarchical Simple Shared Shaping over Ethernet

In Figure 21, the S-VLANs labeled 1, 2, and 3 indicate the possible constituents for S-VLAN 0. The active constituents for the simple shared shaper are the three nodes for S-VLAN 0 in the three traffic-class groups.

| Note: This example uses QoS parameters to configure shared shaping.

1. Configure the traffic classes and traffic-class groups.
   (config)#traffic-class tc1 (config)#exit (config)#traffic-class tc2 (config)#exit (config)#traffic-class-group g1 (config-traffic-class-group)#traffic-class tc1 (config-traffic-class-group)#exit (config)#traffic-class-group g2 extended (config-traffic-class-group)#traffic-class tc2 (config-traffic-class-group)#exit
2. Configure the parameter definitions.
   (config)#qos-parameter-define vlan-g1-max-rate (qos-parameter-define)#controlled-interface-type vlan (qos-parameter-define)#instance-interface-type vlan (qos-parameter-define)#exit
   (config)#qos-parameter-define svlan-g1-max-rate (qos-parameter-define)#controlled-interface-type svlan (qos-parameter-define)#instance-interface-type svlan (qos-parameter-define)#instance-interface-type ethernet (qos-parameter-define)#exit
   (config)#qos-parameter-define vlan-max-rate (qos-parameter-define)#controlled-interface-type vlan (qos-parameter-define)#instance-interface-type vlan (qos-parameter-define)#instance-interface-type svlan (qos-parameter-define)#exit
   (config)#qos-parameter-define svlan-max-rate (qos-parameter-define)#controlled-interface-type svlan (qos-parameter-define)#instance-interface-type svlan (qos-parameter-define)#instance-interface-type ethernet (qos-parameter-define)#exit
3. Configure the shared shaper by referencing parameter definitions in the shaping-rate command.
   (config)#scheduler-profile vlan-be (config-scheduler-profile)#shared-shaping-rate vlan-max-rate simple (config-scheduler-profile)#exit (config)#scheduler-profile svlan-be (config-scheduler-profile)# shared-shaping-rate svlan-max-rate simple (config-scheduler-profile)#exit
   (config)#scheduler-profile svlan-g1 (config-scheduler-profile)#shaping-rate svlan-g1-max-rate (config-scheduler-profile)#exit (config)#scheduler-profile vlan-g1 (config-scheduler-profile)#shaping-rate vlan-g1-max-rate (config-scheduler-profile)#exit (config)#scheduler-profile svlan-g2 (config-scheduler-profile)#shaping-rate svlan-max-rate % 50 (config-scheduler-profile)#exit
4. Configure the QoS profile.
   (config)#qos-profile svlan-4.1 (config-qos-profile)#vlan queue traffic-class best-effort (config-qos-profile)#vlan node scheduler-profile vlan-be (config-qos-profile)#svlan node scheduler-profile svlan-be (config-qos-profile)#vlan queue traffic-class tc1 (config-qos-profile)#svlan node scheduler-profile svlan-g1 group g1 (config-qos-profile)#svlan queue traffic-class tc2 (config-qos-profile)#svlan node scheduler-profile svlan-g2 group g2 (config-qos-profile)#ethernet group g2 scheduler-profile default
5. Attach the QoS profile to the S-VLANs on Fast Ethernet interface 11/0.
   (config)#interface fastEthernet 11/0 (config-if)#svlan 0 qos-parameter svlan-max-rate 4000000 (config-if)#svlan 0 qos-profile svlan-4.1 (config-if)#encapsulation vlan (config-if)#exit
   (config)#interface fastEthernet 11/0.1 (config-if)#svlan id 0 1 (config-if)#ip address 1.2.1.1 255.255.255.0 (config-if)#exit
   (config)#interface fastEthernet 11/0.2 (config-if)#svlan id 0 2 (config-if)#ip address 1.3.1.1 255.255.255.0 (config-if)#exit

#### Related Documentation

- Configuring Simple Shared Shaping
- Simple Shared Shaping Overview