Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Policy Rule Precedence

# next-interface

#### Syntax

[ no ] [ suspend ] next-interface interfaceType interfaceSpecifier
[ next-hop nextHop ] [ classifier-group claclName ] [ precedence precValue ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines an output interface for an IP policy list. When the interfaceType is a broadcast medium, specify a next hop using the next-hop command. The no version removes a next interface rule from a policy list; the suspend keyword temporarily suspends the rule; the no suspend version resumes application of a suspended rule. For IP interfaces, this command is supported only on input policies.

| Note: The next-interface command has been replaced by the forward interface command and may be removed completely in a future release. The SRP module Fast Ethernet port cannot be the destination of the next-interface command.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- nextHop—Next-hop IP address
- claclName—In Policy List Configuration, specifies the classifier control list used to classify packets for this next-hop policy. If you do not specify a classifier group, the router selects all packets from the interface associated with this policy list for this rule.
- precValue—In Policy List Configuration, specifies the precedence of this rule in relation to other rules within this set

#### Mode

Classifier Group Configuration, Policy List Configuration

## Related Documentation

- Policy Rule Precedence

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out