# show vlan profile

#### Syntax

show vlan [ bulk-config ] profile [ { interfaceType } interfaceSpecifier ] override
[ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
bulk-config keyword and interfaceType variable added in JunosE Release 7.3.0.

#### Description

Displays information about overriding profile assignments for the bulk-configured VLAN ranges on a VLAN subinterface. Information about base profile assignments is not displayed. You can display information for all VLAN ranges on the router, for all VLAN ranges on a particular VLAN subinterface, or for the VLAN range associated with a particular bulk configuration name.

#### Options

- bulk-config—Displays information about bulk-configured ranges
- interfaceType—One of the following interface types listed in Interface Types and Specifiers:
  - fastEthernet
  - gigabitEthernet
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec