# mpls ldp discovery transport-address

#### Syntax

mpls ldp discovery transport-address ipAddress

no mpls ldp discovery transport-address

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies an arbitrary IP address to be used as the transport address of the local peer advertised in LDP discovery hello messages for interfaces that use the platform label space. The peer router uses the transport address to establish the session TCP connection. By default, the router ID is advertised as the transport address. The no version restores the default transport address, the LSR router ID.

#### Options

- ipAddress—IP address advertised as the transport address

#### Mode

Router Configuration