# color-aware

#### Syntax

[ no ] color-aware

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Configures rate-limit profile to operate in color-aware mode. (Supported only on hierarchical rate limits.) Color-aware rate limits can change the algorithm used depending on the color of the incoming packet, which might have been set in the previous rate limit, in a policy action, or in an earlier policy. The no version restores the default value, which is not color-aware.

#### Mode

Rate Limit Profile Configuration

#### Related Documentation

- Creating a Two-Rate Rate-Limit Profile