# Monitoring LDP-Related Settings for VPLS

#### Purpose

Display MPLS configuration information for a VPLS instance that uses LDP as the signaling protocol.

#### Action

To display information for all VPLS instances configured on the virtual router:

    host1:ve1#show ldp vpls
      Vpls     Vpls   Remote
    Instance    Id      PE      In-label   Out-label
    --------   ----   -------   --------   ---------
    vpls1         1   2.2.2.2         25          27
    vpls2         2   2.2.2.2         26          28

#### Meaning

Table 129 lists the show ldp vpls command output fields.

Table 129: show ldp vpls Output Fields

Field Name | Field Description
--- | ---
Vpls Instance | Name of the VPLS instance for which the configuration information is displayed
Vpls Id | Globally unique identifier for the VPLS domain
Remote PE | IP address of the remote VE (also known as the PE) router
In-label | Incoming MPLS label from the remote site
Out-label | Outgoing MPLS label used to reach the remote site

#### Related Documentation

- show ldp vpls