# monitor atm vc

#### Syntax

monitor atm vc atm interfaceSpecifier vcd [ atm interfaceSpecifier vcd ]*
[ load-interval seconds ] [ display-time-of-day ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays bit rate and packet rate statistics over a specified time interval for one or more ATM virtual circuits (VCs). There is no no version.

#### Options

- interfaceSpecifier—ATM interface specifier; see Interface Types and Specifiers
- vcd—Virtual circuit descriptor that is an identifier for the VC in other commands; number in the range 1–2147483647
- seconds—Number of seconds in the range 5–30 that specifies the time interval at which the router calculates bit rates and packet rates for the specified VC; default value is 5 seconds
- display-time-of-day—Sets time at which the router calculates the bit rate and packet rate statistics for the current interval
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Privileged Exec, User Exec