# suspicious-control-flow-detection protocol threshold

#### Syntax

suspicious-control-flow-detection protocol protocolValue threshold thresholdValue

no suspicious-control-flow-detection protocol protocolValue threshold

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Sets a threshold rate at which a flow becomes suspicious for a specific protocol. The no version restores the default for a protocol, which is a protocol-dependent numeric value.

#### Options

- protocolValue—Name of the protocol
- thresholdValue—Zero or a number in the range 3–65535; when set to zero, no flows for the protocol type are considered suspicious

#### Mode

Global Configuration