# mpls traffic-eng flood thresholds

#### Syntax

mpls traffic-eng flood thresholds { up | down } percentage [ percentage ]*

no mpls traffic-eng flood thresholds { up | down }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies thresholds for the flooding of the current reservable bandwidth throughout the network. You can configure a set of thresholds for increases or decreases in bandwidth. Flooding is triggered when the reservable bandwidth increases past any up threshold or decreases past any down threshold. The no version restores the following default values:

- For increases in bandwidth (up changes)—15, 30, 45, 60, 75, 80, 85, 90, 95, 97, 98, 99, 100
- For decreases in bandwidth (down changes)—100, 99, 98, 97, 96, 95, 90, 85, 80, 75, 60, 45, 30, 15

#### Options

- up—Specifies that an increase in bandwidth past the threshold triggers flooding
- down—Specifies that a decrease in bandwidth past the threshold triggers flooding
- percentage—Percentage of reservable bandwidth, a value from 1 to 100 percent for increasing bandwidth and from 0 to 99 percent for decreasing bandwidth
- *—Indicates that the percentage can be repeated multiple times in a list in the command line

#### Mode

Interface Configuration, Subinterface Configuration