Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring a Dynamic Interface from a Profile in Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass

# Enabling Multiclass MLPPP

You can enable multiclass MLPPP on an MLPPP interface and create a specified number of multilink classes on it. A maximum number of eight multilink classes are supported per MLPPP interface.

Before you enable multiclass MLPPP:

- Define the QoS traffic classes

  See Configuring Traffic Classes That Define Service Levels.

To enable multiclass MLPPP and create a specified number of multilink classes on a dynamic MLPPP interface:

1. From Global Configuration mode, create an MLPPP dynamic profile by assigning it a name.
   host1(config)#profile ppp-multilink-profile
2. Enable multiclass MLPPP and specify the number of multilink classes to create.
   host1(config-profile)#ppp multilink multiclass multilink-classes 8

To enable multiclass MLPPP and create a specified number of multilink classes on a static MLPPP interface:

1. From Global Configuration mode, specify the individual interface on which you want to configure multiclass MLPPP.
   host1(config)#interface gigabitEthernet 3/0/0
2. Specify PPPoE as the encapsulation method on the interface.
   host1(config-if)#encapsulation pppoe
3. Create a PPPoE subinterface.
   host1(config)#interface gigabitEthernet 3/0/0.10
4. Specify MLPPP as the encapsulation method on the subinterface.
   host1(config-if)#encapsulation mlppp
5. Enable multiclass MLPPP and specify the number of miltilink classes to create.
   host1(config-if)#ppp multilink multiclass multilink-classes 8

## Related Documentation

- Configuring a Dynamic Interface from a Profile in Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass

#### Published: 2011-03-28

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out