# ipv6 pim ssm

#### Syntax

ipv6 pim ssm { default | range ipv6AccessList }

no ipv6 pim ssm

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables SSM and defines the SSM range of IPv6 multicast addresses. The no version disables SSM on the router.

#### Options

- default—Specifies that SSM use the IANA-specified range of 232/8
- ipv6AccessList—Name of the IPv6 access list that specifies the range of multicast addresses you want SSM to use

#### Mode

Global Configuration