# mpls lsp retries

#### Syntax

mpls lsp retries retryNum

no mpls lsp retries

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the number of attempts that will be made to set up an LSP for RSVP-TE after a failure other than one due to no available route. The no version restores the default value, 0, which means the attempts will be made until successful.

#### Options

- retryNum—Number of retry attempts in the range 0–65535

#### Mode

Global Configuration