# ip ospf transmit-delay

#### Syntax

ip ospf transmit-delay transmDelay

no ip ospf transmit-delay

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the estimated time it takes to transmit a link-state update packet on the interface. The no version restores the default value.

#### Options

- transmDelay—Link-state transmit delay, a number in the range 0–3600 seconds; default value is 1 second

#### Mode

Interface Configuration, Subinterface Configuration