# radius dsl-port-type

#### Syntax

radius dsl-port-type { sdsl | adsl-cap | adsl-dmt | idsl | xdsl | virtual }

no radius dsl-port-type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets RADIUS attribute 61, NAS-Port-Type, in RADIUS access request packets and accounting start and stop packets for ATM interfaces. The no version restores the default setting, xdsl.

#### Options

- sdsl—Symmetric DSL
- adsl-cap—Asymmetric DSL, carrierless amplitude phase modulation
- adsl-dmt—Asymmetric DSL, discrete multitone
- idsl—ISDN DSL
- xdsl—DSL of unspecified type (default)
- virtual—Virtual

#### Mode

Global Configuration