# ppp reassembly

#### Syntax

ppp reassembly [ mrru ]

no ppp reassembly

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables reassembly on an MLPPP link interface and optionally specifies the administrative MRRU value, in octets, for the link. The no version disables reassembly on the link and restores the default value, which is the link’s local MRU.

#### Options

- mrru—Maximum allowable size of the PPP packet payload that the router can receive, in the range 64–65535; default value is the link’s local MRU

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration