Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Monitoring MPLS Layer 2 Interfaces for Layer 2 Services over MPLS in the JunosE BGP and MPLS Configuration Guide

# show mpls interface

#### Syntax

show mpls interface [ major | shim | minor ]
[ summary | [ state not-up ] [ brief | detail ]
[ interfaceType interfaceSpecifier | name tunnelName ] [ delta ] ] [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
minor, detail, and delta keywords added in JunosE Release 7.1.0.
name keyword and tunnelName variable added in JunosE Release 7.1.0.
summary keyword added in JunosE Release 8.0.0.

#### Description

Displays status and configuration information about MPLS major interfaces, shim interfaces, minor interfaces or all MPLS interfaces (the default) on the router.

#### Options

- major—Displays information about MPLS major interfaces
- shim—Displays information about shim interfaces used for layer 2 over MPLS
- minor—Displays information about MPLS minor interfaces
- summary—Displays summary information about MPLS interfaces
- state not-up—Displays information only about interfaces that are not operationally up
- brief—Displays limited interface information
- detail—Displays detailed information
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- tunnelName—Name of the tunnel represented by the MPLS minor interface
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring MPLS Layer 2 Interfaces for Layer 2 Services over MPLS in the JunosE BGP and MPLS Configuration Guide

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out