# ip bgp-community new-format

#### Syntax

[ no ] ip bgp-community new-format

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies that communities must be displayed in AA:NN format, where AA is a number that identifies the autonomous system and NN is a number that identifies the community within the autonomous system. The no version restores the default display.

#### Mode

Global Configuration