# nas-port-type atm

#### Syntax

nas-port-type atm { adsl-cap | adsl-dmt | idsl | sdsl | xdsl | cable | wireless-80211 |
wireless-cdma | wireless-umts | wireless-1x-ev | wireless-other | iapp | value }

no nas-port-type atm

#### Release Information

Command introduced before Release 7.1.0.

#### Description

Specifies the RADIUS NAS-Port-Type attribute (61) used for ATM interfaces. The no version removes the NAS-Port-Type setting.

#### Options

- adsl-cap—Asymmetric DSL, Carrierless Amplitude Phase Modulation
- adsl-dmt—Asymmetric DSL, Discrete Multi-Tone
- idsl—ISDN DSL
- sdsl—Symmetric DSL
- xdsl—DSL of unknown type
- cable—Cable
- wireless-80211—Wireless 802.11
- wireless-cdma—Wireless code division multiple access (CDMA)
- wireless-umts—Wireless universal mobile telecommunications system (UMTS)
- wireless-1x-ev—Wireless 1xEV
- wireless-other—Wireless other
- iapp—Inter Access Point Protocol (IAPP)
- value—Number in the range 0–65535

#### Mode

AAA Profile Configuration