# radius authentication server

#### Syntax

[ no ] radius authentication server ipAddress

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the IP address of a RADIUS authentication server and puts the E Series router into RADIUS Configuration mode. The no version deletes the instance of the RADIUS server.

#### Options

- ipAddress—IP address of the server

#### Mode

Global Configuration