# reaction-factor

#### Syntax

reaction-factor reactionFactor

no reaction-factor

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Specifies the reaction factor for all simple shared shapers on the router. The reaction factor determines how the shared shaper reacts to changes in the measured rate. The no version removes the specified reaction factor from all simple shared shapers on the router.

#### Options

- reaction-factor—Percentage in the range 0–1000; default value is 200

#### Mode

QoS Shared Shaper Control Configuration

#### Related Documentation

- Configuring Simple Shared Shaper Algorithm Variables