# operations-per-hop

#### Syntax

operations-per-hop operationsHopValue

no operations-per-hop

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the number of operations sent to a designated hop before the TTL value is increased. This option applies only to the pathEcho type. The no version restores the default value, 3.

#### Options

- operationsHopValue—Number of operations per hop; default value is 3

#### Mode

RTR Configuration