# receive version

#### Syntax

[ no ] receive version [ 1 ] [ 2 ] [ off ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Restricts the RIP version that the router can receive on a RIP remote-neighbor interface. The no version sets the remote-neighbor interface back to the default value, receiving both RIP version 1 and version 2.

#### Options

- 1—Specifies RIP version 1 only
- 2—Specifies RIP version 2 only
- off—Turns reception off

#### Mode

Remote Neighbor Configuration