# snmp-server interfaces compress

#### Syntax

[ no ] snmp-server interfaces compress [ interfaceLayer ]* table-type TableType

#### Release Information

Command introduced before JunosE Release 7.1.0.

The table-type keyword added in JunosE Release 10.2.0.

#### Description

Removes a set of sublayers from the ifTable, the ifStackTable, and the ipAddrTable. You can enter this command multiple times to remove multiple interfaces. By specifying a table type, you can restrict interface compression only to the specified table types in the SNMP interface configuration. The no version negates the compression.

#### Options

- interfaceLayer—Interface layer that you want to remove from the ifTable, the ifStackTable, and the ipAddrTable. If you do not specify an interface layer, the router removes the following interface layers:
  - ip
  - ppp
  - ethernetSubinterface
  - hdlc
  - pppoeInterface
  - ipLoopback
  - ipVirtual
  - pppLinkInterface
  - slepInterface/ciscoHdlc
- TableType—Table type on the SNMP interface configuration to which you want to limit the interface compression. The supported table types are interface-table and interface-stack-table.
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration