# show ipv6 mroute

#### Syntax

show ipv6 mroute [ groupIpAddress [ sourceIpAddress ] ]
[ summary | count | oif-detail | statistics ] [ active [ bandwidth ] ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
active keyword added in JunosE Release 8.1.0.
oif-detail keyword added in JunosE Release 12.0.0.

#### Description

Displays information about all or specified multicast routes.

#### Options

- groupIpAddress—IPv6 address of a multicast group
- sourceIpAddress—IPv6 address of a multicast source
- summary—Displays brief information about the multicast routes
- count—Displays the number of groups and sources
- oif-detail—Displays details of the join interfaces corresponding to the mapped interface when OIF-mapping is configured
- statistics—Displays statistics for packets received through multicast routes that the router has added to the multicast routing table and established on the appropriate line modules
- active—Displays active mroutes
- bandwidth—Admission bandwidth for active multicast routes that is greater than the specified bandwidth threshold; default is 4000 bps
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Limiting Interface Admission Bandwidth in the JunosE Multicast Routing Configuration Guide
- Limiting Port Admission Bandwidth in the JunosE Multicast Routing Configuration Guide