# baseline atm vp interface

#### Syntax

baseline atm vp interface atm interfaceSpecifier vpi

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for an ATM virtual path (VP) interface. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- interfaceSpecifier—ATM interface specifier; see Interface Types and Specifiers
- vpi—Virtual path identifier of the PVC. The numeric range depends on the line module capabilities and current configuration.

#### Mode

Privileged Exec