Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# path ds1|e1 channel-group description

#### Syntax

path pathChannel { ds1 | e1 } tributaryIdentifier
channel-group channelGroupNumber description name

no path pathChannel { ds1 | e1 } tributaryIdentifier
channel-group channelGroupNumber description

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns a text description or an alias to a DS1 (T1) or an E1 channel group for channelized SONET and SDH interfaces. Use the show controllers sonet command to display the text description. The no version removes the description or alias.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- tributaryIdentifier—Specifier for the tributary in the format
  pathChannel { ds1 | e1 } pathPayload/tributaryGroup/tributaryNumber
  - pathPayload—Payload number for the path; value is 1 for SONET and in the range 1–3 for SDH
  - tributaryGroup—Number, in the range 1–7, that identifies the group within the path
  - tributaryNumber—Number of the tributary within the tributary group; the value is in the range 1–4 if the tributary type is vt15 or tu11 and in the range 1–3 if the tributary type is tu12
- channelGroupNumber—Either a fractional T1 interface in the range 1–24 or a fractional E1 interface in the range 1–31
- name—Text string or alias of up to 80 characters for the DS1 or E1 channel group for channelized SONET and SDH interfaces

#### Mode

Controller Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out