# ipv6 pim query-interval

#### Syntax

ipv6 pim query-interval queryTime

no ipv6 pim query-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies how often the router sends PIM router query messages from this interface. The no version specifies the default time interval, 30 seconds.

#### Options

- queryTime—Interval in the range 0–210 seconds at which the router sends PIM router query messages from this interface

#### Mode

Interface Configuration