# adapter accept

#### Syntax

adapter accept adapterSpecifier

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Erases from NVS the type and configuration of the previous I/O adapter (IOA) in the specified IOA bay, and allows you to configure a new IOA. Issue this command after you have installed a different type of IOA in an IOA bay. You can use this command only when the state of the IOA is not present or disabled (mismatch). There is no no version.

| Note: Issuing this command reboots the line module associated with the IOA, but it does not accept its configuration. To accept the configuration of the line module and its associated IOAs, issue the slot accept command.

#### Options

- adapterSpecifier—Particular IOA in the format slot/adapter:
  - slot—Number of the chassis slot; for E120 routers, in the range 0–5; for E320 routers, in the range 0–5 or 11–16
  - adapter—Identifier for the IOA within the chassis slot, either 0 or 1, where:
    - 0 indicates that the IOA is installed in the right IOA bay (E120 router) or the upper IOA bay (E320 router).
    - 1 indicates that the IOA is installed in the left IOA bay (E120 router) or the lower IOA bay (E320 router).

#### Mode

Global Configuration