Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators
- Creating a QoS Parameter on an Interface Superset or Interface Set

# instance-interface-type

#### Syntax

instance-interface-type {instanceInterfaceType | set | superset }

no instance-interface-type { instanceInterfaceType | all }

#### Release Information

Command introduced in JunosE Release 7.1.0.
lag keyword added in JunosE Release 8.1.0.

set and superset keywords added in JunosE Release 9.2.0.

#### Description

Assigns an instance-interface type to a QoS parameter definition. Instance-interface types indicate the interfaces for which QoS clients can assign QoS parameter instances. You can specify up to eight instance-interface types for each parameter definition. The no version removes the specified instance-interface type from the parameter definition.

#### Options

- instanceInterfaceType—One of the following instance-interface types: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, lag, l2tp-session, l2tp-tunnel, lsp, pppoe, serial, server-port, svlan, vlan
- set—Specifies an interface set as an instance-interface type
- superset—Specifies an interface superset as an instance-interface type
- all—Removes all instance-interface types

#### Mode

QoS Parameter Definition

## Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators
- Creating a QoS Parameter on an Interface Superset or Interface Set

#### Published: 2011-04-07

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out