# member-interface-type

#### Syntax

member-interface-type {vlan | atm-vc | ip}

no member-interface-type

#### Release Information

Command introduced in JunosE Release 9.2.0.

#### Description

Configures the member-interface type for a QoS interface set. The no version removes the member-interface type from the parameter definition.

#### Options

- vlan—Specifies the member-interface-type as VLAN
- atm–vc—Specifies the member-interface-type as VLAN
- ip—Specifies the member-interface-type as VLAN

#### Mode

QoS Interface Set Configuration

#### Related Documentation

- Configuring Interface Sets for QoS