# minimum-links

#### Syntax

minimum-links minimumLinkValue

no minimum-links

#### Release Information

Command introduced in JunosE Release 10.0.0.

#### Description

Configures the minimum number of member links in the link aggregation group (LAG) bundle that must be in the Collecting/Distributing state for the LAG interface to be considered up. The no version resets the minimum number of member links to the default value.

#### Options

- minimumLinkValue—Minimum number of links in the LAG bundle in the range 1-8 (8 is the maximum number of member links per LAG bundle); default value is 1.

#### Mode

Interface Configuration

#### Related Documentation

- Configuring 802.3ad Link Aggregation and Link Redundancy in the JunosE Link Layer Configuration Guide