# area virtual-link transmit-delay

#### Syntax

[ no ] area { areaId | areaIdInt } virtual-link ipAddress transmit-delay transmDelay

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines an OSPF virtual link and the estimated time it takes to transmit a link-state update packet on the virtual link. The no version removes the virtual link's transmit delay.

#### Options

- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value in the range 0–4294967295
- ipAddress—IP address associated with the virtual link neighbor
- transmDelay—LSA transmit delay; an integer in the range 0–3600 seconds; default value is 1 second

#### Mode

Router Configuration