Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# show ipv6 route

#### Syntax

show ipv6 route [ vrf vrfName ] [ ipv6Address [ detail ] | ipv6Prefix [ detail ] ] [ all ]
[ protocol ] [ filter ]

To display summary information:

show ipv6 route summary [ vrf vrfName ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Displays current state of the IPv6 routing table.

#### Options

- vrfName—Name of the VRF
- ipv6Address—IPv6 address
- ipv6Prefix—Prefix of prefix list entry; in the format IPv6baseaddress / length; for example, 1::1/32
- detail—Displays detailed information about the specific route
- all—Displays routes from all sources to a prefix
- protocol—One of the following protocols for which you want to display the best routes in the routing table; no routes are displayed if routes for the specified protocol are not present in the routing table
  - access—Displays the best access-server routes (BGP) in the routing table
  - access-internal—Displays the best access-internal routes in the routing table
  - bgp—Displays the best BGP routes in the routing table
  - bgp-tunnel—Displays the best BGP tunnel routes in the routing table
  - dvmrp—Displays the best DVMRP routes in the routing table
  - isis—Displays the best IS-IS routes in the routing table
  - ldp—Displays the best LDP tunnel routes in the routing table
  - local—Displays the best locally connected routes in the routing table
  - mbgp—Displays the best MBGP routes in the routing table
  - ospf—Displays the best OSPF routes owned by in the routing table
  - other—Displays the best internal control routes in the routing table
  - rip—Displays the best RIP routes in the routing table
  - rsvp—Displays the best RSVP tunnel routes in the routing table
  - static—Displays the best static routes added by network management to the routing table
  - static-rpf—Displays the best static RPF routes added by network management to the routing table
- filter—See Filtering show Commands
- summary—Displays summary counters for all routes in the IPv6 routing table

#### Mode

Privileged Exec, User Exec

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out