Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- QoS for 802.3ad Link Aggregation Interfaces Overview
- Subscriber Load Balancing for 802.3ad Link Aggregation Groups Overview
- Enabling Default Subscriber Load Balancing for 802.3ad Link Aggregation Groups
- interface lag
- member-interface
- node
- qos-profile
- queue

# Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups

The type of load balancing that the system performs depends on the configuration of the scheduler hierarchy in the QoS profile.

To configure the scheduler hierarchy for subscriber load balancing:

1. Configure the QoS profile.
   host1(config)#qos-profile subscriber-lag
2. Configure the queues and nodes for VLANs and S-VLANs.
   host1(config-qos-profile)#vlan queue traffic-class best-effort host1(config-qos-profile)#vlan queue traffic-class tc1 host1(config-qos-profile)#vlan node scheduler-profile subscriber host1(config-qos-profile)#svlan node scheduler-profile svlan host1(config-qos-profile)#svlan node group g1 scheduler-profile svlan
3. Create the LAG interface and assign member interfaces.
   host1(config)#interface lag lg1 host1(config-if)#member-interface gigabitEthernet 3/0 host1(config-if)#member-interface gigabitEthernet 3/1
4. Attach the QoS profile to the LAG interface.
   host1(config-if)#qos-profile subscriber-lag

## Related Documentation

- QoS for 802.3ad Link Aggregation Interfaces Overview
- Subscriber Load Balancing for 802.3ad Link Aggregation Groups Overview
- Enabling Default Subscriber Load Balancing for 802.3ad Link Aggregation Groups
- interface lag
- member-interface
- node
- qos-profile
- queue

#### Published: 2011-03-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out