Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Monitoring BGP-Related Settings for L2VPNs in the JunosE BGP and MPLS Configuration Guide

# show ip bgp advertised-routes

#### Syntax

To display routes advertised to a neighbor or peer group in all address families or a particular address family:

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName |
l2vpn [ all ] | route-target signaling ]
{ neighbors { ipAddress | ipv6Address } | peer-group peerGroupName }
advertised-routes [ fields { fieldOptions } ] [ delta ] [ filter ]

To display routes advertised to the specified peer group for all VPN address families or for a particular VPN address family after the application of route-target filters advertised by the specified member of the peer group:

show ip bgp [ vpnv4 all | vpnv4 vrf vrfName ] | l2vpn [ all ] | route-target signaling ]
peer-group peerGroupName advertised-routes
route-target-filter neighbor { ipRtfNbrAddress| ipv6RtfNbrAddress }
[ fields { pgfieldOptions } ] [ delta ] [ filter ]

To display the route that best matches the specified address for all address families or for a particular address family; not available for the L2VPN address family:

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName ]
{ neighbors { ipAddress | ipv6Address } | peer-group peerGroupName }
advertised-routes network [ networkMask [ longer-prefixes ] ]
[ fields { fieldOptions } ] [ delta ] [ filter ]

To display routes advertised to a neighbor or peer group with the specified site ID and block offset in the L2VPN address family:

show ip bgp l2vpn all
{ neighbors { ipAddress | ipv6Address } | peer-group peerGroupName }
advertised-routes site-id siteId block-offset blockOffset
[ fields { fieldOptions } ] [ delta ] [ filter ]

To display all routes or the route that best matches the specified address advertised to a neighbor or peer group in only the route-target address family:

show ip bgp route-target signaling
{ neighbors { ipAddress | ipv6Address } | peer-group peerGroupName }
advertised-routes rtfPrefix [ longer-prefixes ]
[ fields { fieldOptions} ] [ delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
l2vpn and all keywords added in JunosE Release 7.1.0.
site-id keyword and siteId variable added in JunosE Release 7.1.0.
block-offset keyword and blockOffset variable added in JunosE Release 7.1.0.
ipv6Address variable added in JunosE Release 8.0.0.
route-target signaling and route-target-filter neighbor keywords and ipRtfNbrAddress, ipv6RtfNbrAddress, and rtMemNlri variables added in JunosE Release 8.2.0.
rtMemNlri variable replaced by rtfPrefix variable in JunosE Release 9.1.0.

#### Description

Displays the routes in the Adj-RIBs-Out table of the specified peer or peer group. For peers, displays routes that have been previously advertised to the peer and the attributes for the routes before the application of outbound policy.

For peer groups, displays routes that will be advertised to the peer group, but includes the full set of route attributes associated with the routes after the application of outbound policy. This command returns an error message unless you first enable rib-out with the no neighbor rib-out disable command or the no rib-out disable command.

#### Options

- ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
- ipv4 multicast—Specifies the IPv4 multicast address family and routing table
- vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
- vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
- l2vpn all—Displays information for only the L2VPN address family; the all keyword is optional unless you specify a site ID and block offset
- route-target signaling—Specifies the route-target address family
- ipAddress—IP address of a neighbor whose routes the router has learned
- ipv6Address—IPv6 address of a neighbor whose routes the router has learned
- peerGroupName—Name of a BGP peer group
- route-target-filter neighbor—Displays routes actually advertised to the specified peer group member (neighbor); which routes are advertised is determined by the application of the route-target filter received from that neighbor to routes in the peer group’s Adj-RIBs-Out table
- ipRtfNbrAddress—IP address of a peer group member that has advertised route-target membership filtering information
- ipv6RtfNbrAddress—IPv6 address of a peer group member that has advertised route-target membership filtering information
- network—Route that best matches this IP address; if no network is specified, displays the fields for all networks
- networkMask—Address mask to be applied to the network address
- longer-prefixes—Displays all routes with a prefix that is equal to or more specific than the specified prefix
- siteId—Numerical identifier for the site; must be an unsigned 16-bit integer greater than zero that is unique across the VPLS domain
- blockOffset—Integer in the range 1–65535 that identifies a block offset for which information is displayed
- rtfPrefix—Prefix representing the route-target membership NLRI (RT-MEM-NLRI), in the format asNumber:extendedCommunity/prefixLength (for example, 320:320:524/36) where:
  - asNumber—AS number for origin of route target information, in the range 1–4294967295
  - extendedCommunity—Two-part number in the format number1:number2 that identifies an extended community of VPNs, in the format number1:number2, where:
    - number1—Autonomous system (AS) number, in the range 1–4294967295, or an IP address
    - number2—Unique integer, in the range 1–4294967295; 32 bits if number1 is a 16-bit AS number; 16 bits if number1 is an IP address or a 32-bit AS number
  - prefixLength—Number that specifies the length of the route prefix, in the range 32–96
- fields—Displays only the specified fields; the display order of the fields is hard-coded and not affected by the order in which you enter them
- fieldOptions—Fields to be displayed, in the format
  all | [ afi | aggregator | as-path | atomic-aggregate | best | clusters | communities | extended-communities | imported | intro | in-label | loc-pref | med | next-hop | next-hop-cost | origin | originator-id | out-label | peer | peer-type | rd | safi | stale | unknown-types | weight ]*
  - all—All available information; not recommended, because this information for each network does not fit on a single line and is difficult to read
  - afi—Address family identifier
  - aggregator—AS number and IP address of aggregator
  - as-path—AS path through which this route bas been advertised
  - atomic-aggregate—Whether the atomic aggregate attribute is present
  - best—Whether this is the best route for the prefix
  - clusters—List of cluster IDs through which the route has been advertised
  - communities—Community number associated with the route
  - extended-communities—Extended community
  - imported—Whether the route was imported
  - intro—Introductory information about the state of various BGP attributes; this information is displayed only if you specify this keyword
  - in-label—MPLS label for the route; the label received with incoming MPLS frames; typically, but not always, this is the label advertised to MP-BGP peers
  - loc-pref—Local preference for the route
  - med—Multiexit discriminator for the route
  - next-hop—IP address of the next router that is used when forwarding a packet to the destination network
  - next-hop-cost—Whether the indirect next hop of the route is unreachable, if not, displays IGP cost to the indirect next hop
  - origin—Origin of the route
  - originator-id—Router ID of the router in the local AS that originated the route
  - out-label—MPLS label for the route; the label sent with outgoing MPLS frames; also the label received from MP-BGP peer; typically, but not always, this is the label received from MP-BGP peers
  - peer—IP address of BGP peer from which route was learned
  - peer-type—Type of BGP peer: internal, external, or confederation
  - rd—Route distinguisher
  - safi—Subsequent address family identifier
  - stale—Route that has gone stale due to peer restart
  - unknown-types—Attribute codes for unknown path attributes
  - weight—Weight of the route
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring BGP-Related Settings for L2VPNs in the JunosE BGP and MPLS Configuration Guide

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out