# radius vlan nas-port-format stacked

#### Syntax

radius vlan nas-port-format stacked

no radius vlan nas-port-format

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the RADIUS NAS-Port attribute to include the S-VLAN ID, in addition to the VLAN ID, for subscribers on Ethernet interfaces. The no version restores the default situation, which does not include the S-VLAN ID.

#### Mode

Global Configuration