# radius rollover-on-reject

#### Syntax

radius rollover-on-reject { enable | disable }

no radius rollover-on-reject

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

On a virtual router, specifies whether the router should roll over to the next RADIUS server when the router receives an access-reject message for the user it is authenticating. The no version restores the default value, disable.

#### Options

- enable—Specifies the feature
- disable—Disables the feature; this is the default setting

#### Mode

Global Configuration