# mark-de

#### Syntax

[ no ] [ suspend ] mark-de deValue

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Marks the DE bit in the Frame Relay header of packets matching the current classifier control list. The no version removes the mark rule from a policy list; the suspend version temporarily suspends a mark rule; the no suspend version resumes application of a suspended rule.

| Note: This command replaces the Policy List Configuration version of the mark-de command, which may be removed completely in a future release.

#### Options

- deValue—Value of the DE bit; 0 or 1

#### Mode

Classifier Group Configuration

#### Related Documentation

- Assigning Values to the ATM CLP Bit
- Policy Rule Precedence