[Contents] [Prev] [Next] [Index] [Report an Error]

# Environmental Requirements

See System Specifications for complete environmental specifications.

Choose a location for the router that is dry, relatively dust free, well ventilated, and air conditioned. If you install equipment in a rack, be sure that the floor is capable of supporting the combined weight of the rack and the installed equipment. Place the router in a location with sufficient access to power and network cables.

Like other network devices, the router generates a significant amount of heat. You must provide a balanced environment so that the router performs properly and safely. See System Specifications for acceptable ranges of temperature and humidity.

Be sure to allow enough space around the router for adequate ventilation. Inadequate ventilation can cause the system to overheat.

| Caution: Do not block the air vents on the router. Otherwise, the router might overheat.

[Contents] [Prev] [Next] [Index] [Report an Error]