> - Download PDFs
> - service dhcp-local

> # service dhcp-local

> #### Syntax

> [ no ] service dhcp-local [ equal-access | standalone [ authenticate ] ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Enables the DHCP local server. In standalone mode, the authenticate keyword enables AAA-based authentication for incoming DHCP clients. The no version disables the DHCP local server and does not save the previous settings.

> #### Options

> - equal-access—Enables the DHCP local server to work with the SRC (formerly SDX or SSC) or HTTP local server for non-PPP equal access, the default option
> - standalone—Configures the router as a DHCP local server
> - authenticate—Enables AAA-based authentication of incoming DHCP clients

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.