[Contents] [Prev] [Next] [Index] [Report an Error]

## mplsShimInterface

#### Description

MPLS Shim Interface events

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Signaling protocol interaction failures; shim interface engine interaction failures; shim interface finite state machine bad state transitions; shim interface configuration errors

#### Warning Log

None

#### Notice Log

None

#### Info

None

#### Debug

Shim interface finite state machine transitions; signaling protocol interaction; shim interface to engine transactions; shim interface configuration transactions

#### Filter

router virtualRouterName [ interface interfaceType interfaceSpecifier ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of the virtual router for which you want to log events
- interface—Logs events on a specific interface on the virtual router
- interfaceType—Type of the interface for which you want to log events. For example, atm.
- interfaceSpecifier—Location of the interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]