> - Download PDFs
> - radius rollover-on-reject

> # radius rollover-on-reject

> #### Syntax

> radius rollover-on-reject { enable | disable }

> no radius rollover-on-reject

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> On a virtual router, specifies whether the router should roll over to the next RADIUS server when the router receives an access-reject message for the user it is authenticating. The no version restores the default value, disable.

> #### Options

> - enable—Specifies the feature
> - disable—Disables the feature; this is the default setting

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.