> - Download PDFs
> - show radius nas-port-format extended

> # show radius nas-port-format extended

> #### Syntax

> show radius nas-port-format extended { atm | ethernet } [ filter ]

> #### Release Information

> Command introduced in JUNOSe Release 7.1.0.

> #### Description

> Displays the format used for RADIUS attribute 5, NAS-Port, on the E120 router and the E320 router.

> #### Options

> - atm—Displays information about ATM interfaces
> - ethernet—Displays information about Gigabit Ethernet and 10-Gigabit Ethernet interfaces
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.