[Contents] [Prev] [Next] [Index] [Report an Error]

## bgpRoutes

#### Description

BGP routing table updates

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

Failure to add, remove, or modify BGP route in IP forwarding table

#### Notice Log

BGP route added to, removed from, or modified in the IP forwarding table; aggregate route added to, removed from, or modified in Loc-RIB; network route added to, removed from, or modified in Loc-RIB; best route for internal peers for a given prefix became available; best route for internal peers for a given prefix is no longer available, has changed, or has become available; best route for external peers for a given prefix is no longer available, has changed, or has become available; MPLS base tunnel used to reach an indirect next-hop came up or went down; MPLS stacked tunnel for label came up; indirect next-hop became reachable or unreachable; direct next-hop for an indirect next-hop changed; MPLS tunnel for Inter-AS label came up or went down; route added to L2VPN instance; route deleted from L2VPN instance; route modified for L2VPN instance; -VE device for multihomed local layer 2 site 1 changed from peer to peer2

#### Info

None

#### Debug

Redistributed route added to, removed from, or modified in Loc-RIB; advertisement for a given prefix received; withdraw for a given prefix received; local route-target-filtering route added to or removed from prefix in addressFamily

#### Filter 1

access-class accessClassName [ route-map routeMapName routeMapOptions | filtering-router filteringRouterName filteringRouterOptions | in | out ]

- access-class—Logs events for traffic that matches a specific access class
- accessClassName —Name of the access class for which you want to log events
- route-map—Logs events for traffic that matches a specific route map
- routeMapName—Name of route map for which you want to log events
- routeMapOptions—In the following format—filtering-router filteringRouterName filteringRouterOptions | in | out
- filtering-router—Logs events only if the access class or route map are defined on a specific virtual router
- filteringRouterName—Virtual router where the access class or route map or both are defined
- filteringRouterOptions—in | out
- in—Matches on traffic coming into the access class, route map, or virtual router
- out—Matches on traffic sent out of the access class, route map, or virtual router

#### Filter 2

peer peerIpAddress | peerIpv6Address
[ access-class accessClassName accessClassOptions |
route-map routeMapName routeMapOptions |
filtering-router filteringRouterName filteringRouterOptions | in | out ]

- peer—Logs events for traffic that matches a specific peer
- peerIpAddress—IP address of the peer for which you want to log events
- peerIpv6Address—IPv6 address of the peer for which you want to log events
- access-class—Logs events for traffic that matches a specific access class
- accessClassName—Name of the access class for which you want to log events
- accessClassOptions—In the following format—filtering-router filteringRouterName filteringRouterOptions | in | out
- route-map—Logs events for traffic that matches a specific route map
- routeMapName—Name of route map for which you want to log events
- routeMapOptions—In the following format—filtering-router filteringRouterName filteringRouterOptions | in | out
- filtering-router—Logs events only if the peer, access class or route map are defined on a specific virtual router
- filteringRouterName—Virtual router where the peer, access class or route map or both are defined
- filteringRouterOptions—in | out
- in—Matches on traffic coming into the peer, access class, route map, or virtual router
- out—Matches on traffic sent out of the peer, access class, route map, or virtual router

#### Filter 3

route-map routeMapName
[ filtering-router filteringRouterName filteringRouterOptions | in | out ]

- route-map—Logs events for traffic that matches a specific route map
- routeMapName—Name of route map for which you want to log events
- filtering-router—Logs events only if the route map is defined on a specific virtual router
- filteringRouterName—Virtual router where the route map is defined
- filteringRouterOptions—in | out
- in—Matches on traffic coming into the route map or virtual router
- out—Matches on traffic sent out of the route map or virtual router

#### Filter 4

router virtualRouterName [ access-class accessClassName accessClassOptions | route-map routeMapName routeMapOptions |
filtering-router filteringRouterName filteringRouterOptions |
peer peerIpAddress peerOptions | in | out ]

- router—Logs events for traffic on a specific virtual router
- virtualRouterName—Name of virtual router
- access-class—Logs events for traffic that matches a specific access class on the specified router
- accessClassName—Name of the access class for which you want to log events
- accessClassOptions—In the following format—route-map routeMapName routeMapOptions | virtual-router virtualRouterName virtualRouterOptions | in | out
- route-map—Logs events for traffic that matches a specific route map
- routeMapName—Name of route map for which you want to log events
- routeMapOptions—In the following format—virtual-router virtualRouterName virtualRouterOptions | in | out
- filtering-router—Logs events only if the access class or route map is defined on a specific virtual router
- filteringRouterName—Virtual router where the access class or route map is defined
- filteringRouterOptions—In the following format—in | out
- peer—Logs events for traffic that matches a specific peer
- peerIpAddress—Address of the peer for which you want to log events
- peerOptions—In the following format—access-class accessClassName accessClassOptions | filtering-router filteringRouterName filteringRouterOptions | route-map routeMapName routeMapOptions | in | out
- in—Matches on traffic coming into the virtual router, access class, or route map
- out—Matches on traffic sent out of the virtual router, access class, or route map

#### Filter 5

in—Matches on traffic coming into the router

#### Filter 6

out—Matches on traffic going out of the router

[Contents] [Prev] [Next] [Index] [Report an Error]